File containing BUFR descriptors to decode (argument to --param):

001001 WMO BLOCK NUMBER [NUMERIC]
001002 WMO STATION NUMBER [NUMERIC]
001015 STATION OR SITE NAME [CCITTIA5]
010051 PRESSURE REDUCED TO MEAN SEA LEVEL [PA]
012101 TEMPERATURE/DRY-BULB TEMPERATURE [K]
011001 WIND DIRECTION [DEGREE TRUE]
011002 WIND SPEED [M/S]

Output:

Message 1 ISMD42 EDZW 020600
Subset 1
1 001001 10 WMO BLOCK NUMBER [NUMERIC]
2 001002 28 WMO STATION NUMBER [NUMERIC]
3 001015 Sankt Peter-Ord STATION OR SITE NAME [CCITTIA5]
4 010051 101360 PRESSURE REDUCED TO MEAN SEA LEVEL [PA]
5 012101 291.15 TEMPERATURE/DRY-BULB TEMPERATURE [K]
6 011001 110 WIND DIRECTION [DEGREE TRUE]
7 011002 6.2 WIND SPEED [M/S]
Subset 2
1 001001 10 WMO BLOCK NUMBER [NUMERIC]
2 001002 129 WMO STATION NUMBER [NUMERIC]
3 001015 Bremerhaven STATION OR SITE NAME [CCITTIA5]
4 010051 101280 PRESSURE REDUCED TO MEAN SEA LEVEL [PA]
5 012101 291.85 TEMPERATURE/DRY-BULB TEMPERATURE [K]
6 011001 110 WIND DIRECTION [DEGREE TRUE]
7 011002 4.1 WIND SPEED [M/S]
Subset 3
1 001001 10 WMO BLOCK NUMBER [NUMERIC]
2 001002 261 WMO STATION NUMBER [NUMERIC]
3 001015 Seehausen STATION OR SITE NAME [CCITTIA5]
4 010051 101570 PRESSURE REDUCED TO MEAN SEA LEVEL [PA]
5 012101 291.55 TEMPERATURE/DRY-BULB TEMPERATURE [K]
6 011001 120 WIND DIRECTION [DEGREE TRUE]
7 011002 4.9 WIND SPEED [M/S]
Subset 4
1 001001 10 WMO BLOCK NUMBER [NUMERIC]
2 001002 291 WMO STATION NUMBER [NUMERIC]
3 001015 Angermuende STATION OR SITE NAME [CCITTIA5]
4 010051 101730 PRESSURE REDUCED TO MEAN SEA LEVEL [PA]
5 012101 291.45 TEMPERATURE/DRY-BULB TEMPERATURE [K]
6 011001 100 WIND DIRECTION [DEGREE TRUE]
7 011002 2 WIND SPEED [M/S]
Subset 5
...