QC1 on Geonor bucket content RA

Applies to equipmenttypeid=7 and equipmentmodel like 'GEONOR%'.

Every sensor will have one entry in table checks with

stationid=sensor_info.stationid

qcx=QC1-1-104

medium_qcx=QC1-1

checkname=RANGE_CHECK

checksignature=obs;RA;;|meta;RA_max,RA_highest,RA_high,RA_low,RA_lowest,RA_min;;

and one corresponding row in table station_param

qcx=QC1-1-104

metadata=max;highest;high;low;lowest;min: <a>;<b>;<b>;-3.0;-3.0;-3.0 where <a>, <b>, and <b> is equipmentmodel specific.

GEONOR T200 : <a> = 615, <b> = 500

GEONOR T200B : <a> = 615, <b> = 500

GEONOR T200BM : <a> = 1100, <b> = 900

GEONOR T200BMD : <a> = 1600, <b> = 1400