QC1 on Geonor bucket content RA

Applies to sensor_info.measurement_methodid=217502 and equipmentmodel.description starts with an integer <V>.

Every sensor will have one entry in table checks with

stationid=sensor_info.stationid

qcx=QC1-1-104

medium_qcx=QC1-1

checkname=RANGE_CHECK

checksignature=obs;RA;;|meta;RA_max,RA_highest,RA_high,RA_low,RA_lowest,RA_min;;

and one corresponding row in table station_param

qcx=QC1-1-104

metadata=max;highest;high;low;lowest;min: <V>+115;<V>;<V>;-3.0;-3.0;-3.0 where <a>, <b>, and <b> is equipmentmodel specific.