QC2d-4 Statistics Method Parameter Value

Description of Method

Quality Control Level

QC2d-4

Run Parameters

It shall be possible to run the algorithm for

FF

Characteristics of the data to which the method is applied

CONTROLINFO AND/OR USEINFO

none

TYPEID, PARAMIDS, OTHER METADATA

all typeid

Flag Settings

SPECIFICATION OF CONTROLFLAGS TO BE SET FOR EXPECTED RESULTS OF THE ALGORITHM, I.E. CONSIDER BOTH POSITIVE AND NEGATIVE RESULTS

fstat=1 on no error detection

fstat=2 on error detection

EXPECTIONS OF THE USEINFO FLAGS CORRESPONDING TO CONTROLINFO FLAG SETTINGS

fstat=2 -> useinfo(2)=2

Dependencies

Definition of neighbour station

Definition of regions and related region reference station

Extracts from KDVH