N_1850-2005_AEROSLO_CNONL502

Model-run description for a simulation with CAM4-Oslo (NorESM1-M)

Purpose of simulation: Model validation for PI conditions including chemistry

Contact person: Dirk Olivié (dirk.olivie@met.no)

Data owner: Dirk Olivié (dirk.olivie@met.no)

Revision Number: r155/156

Ensemble runs: No

Production computer used: Cray XT in Bergen (hexagon)

Production date: December 2012 -- April 2013

Storage locations: NorStore (/norstore_osl/projects/NS2345K/noresm/case/N_1850_AEROSLO_CNONL101/)

MET Norway (local disk)

Storage space:

Projects: EarthClim

Publications:

Papers in preparation:

Simulation name(s): N_1850_AEROSLO_CNONL101

Compset name used: N_1850_AEROSLO_CNONL101

Model type: Coupled

Type of run: Hybrid

Simulation period: 174 years

Spin-up period:

Initialisation: Pre-industrial simulation NAER1850CNOC_f19_g16_05 (date 0700-01-01)

Resolution: f19_g16= 1.8×2.5 (atmosphere), ...x... (ocean)

Emission year(s): 1850 (aerosols and precursors)

Emission inventories ACCMIP from IPCC AR5

Greenhouse gases: Prescribed concentrations

Frequency for output: Monthly

Active/changing forcing agents:

Special considerations:

Tuning parameters which are changed relative to the host model CAM4: