Fluxes crossing boundaries

NorESM can simulate several biogeochemical cycles. Here is a list of the fluxes which cross boundaries in the models and how to enable/disable interactions

Component	Source	Receiver	How to enable
Dust	CLM	CAM	Always calculated by CLM. Picked up and used if aerosol scheme is MAM or OSLO_AERO
Dust	CAM	HAMMOC	Leaves CAM as cam_out%dstwet{n},cam_out%dstdry{n}(n=1-4), picked up by HAMMOC in coupler
DMS	HAMMOC	CAM	Enabled automatically in HAMMOC in