Message 1
Subset 1
1 001007 260 SATELLITE IDENTIFIER [CODE TABLE]
2 025060 92 SOFTWARE IDENTIFICATION (SEE NOTE 2) [NUMERIC]
3 001033 85 IDENTIFICATION OF ORIGINATING/GENERATING CENTRE [CODE TABLE]
4 002048 9 SATELLITE SENSOR INDICATOR [CODE TABLE]
5 002048 10 SATELLITE SENSOR INDICATOR [CODE TABLE]
6 005040 32310 ORBIT NUMBER [NUMERIC]
201134 CHANGE DATA WIDTH
7 007001 1353685 HEIGHT OF STATION (SEE NOTE 1) [M]
201000 CANCEL CHANGE DATA WIDTH
202131 CHANGE SCALE
8 007005 0.667 HEIGHT INCREMENT [M]
202000 CANCEL CHANGE SCALE
9 004001 2008 YEAR [YEAR]
10 004002 12 MONTH [MONTH]
11 004003 11 DAY [DAY]
12 004004 19 HOUR [HOUR]
13 004005 24 MINUTE [MINUTE]
14 004007 23.991058 SECONDS WITHIN A MINUTE (MICROSECOND ACCURACY) [SECOND]
15 005001 64.62657 LATITUDE (HIGH ACCURACY) [DEGREE]
16 006001 156.6758 LONGITUDE (HIGH ACCURACY) [DEGREE]
17 008029 3 REMOTLY SENSED SURFACE TYPE [CODE TABLE]
18 008074 0 ALTIMETER ECHO TYPE [CODE TABLE]
19 008012 1 LAND/SEA QUALIFIER [CODE TABLE]
20 025095 0 ALTIMETER STATE FLAG [FLAG TABLE]
21 025096 4 RADIOMETER STATE FLAG [FLAG TABLE]
22 025097 0 THREE DIMENSIONAL ERROR ESTIMATE OF THE NAVIGATOR ORBIT [CODE TABLE]
204001 ADD ASSOCIATED FIELD
23 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
24 999999 1 ASSOCIATED FIELD [NUMERIC]
25 022070 4.39 SIGNIFICANT WAVE HEIGHT [M]
204000 ADD ASSOCIATED FIELD
26 008023 10 FIRST ORDER STATISTICS [CODE TABLE]
27 022070 2.45 SIGNIFICANT WAVE HEIGHT [M]
28 021128 20 NUMBER OF VALID POINTS PER SECOND USED TO DERIVE PREVIOUS PARAME [NUMERIC]
29 008076 0 TYPE OF BAND [CODE TABLE]
204001 ADD ASSOCIATED FIELD
30 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
201129 CHANGE DATA WIDTH
31 999999 1 ASSOCIATED FIELD [NUMERIC]
32 021062 0.52 BACKSCATTER [dB]
201000 CANCEL CHANGE DATA WIDTH
204000 ADD ASSOCIATED FIELD
33 008023 10 FIRST ORDER STATISTICS [CODE TABLE]
34 021062 0.06 BACKSCATTER [dB]
204001 ADD ASSOCIATED FIELD
35 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
201134 CHANGE DATA WIDTH
36 999999 1 ASSOCIATED FIELD [NUMERIC]
37 007001 1353420 HEIGHT OF STATION (SEE NOTE 1) [M]
201000 CANCEL CHANGE DATA WIDTH
204000 ADD ASSOCIATED FIELD
202131 CHANGE SCALE
38 007005 0.142 HEIGHT INCREMENT [M]
202000 CANCEL CHANGE SCALE
39 008023 10 FIRST ORDER STATISTICS [CODE TABLE]
202131 CHANGE SCALE
40 007001 0.703 HEIGHT OF STATION (SEE NOTE 1) [M]
202000 CANCEL CHANGE SCALE
41 021128 20 NUMBER OF VALID POINTS PER SECOND USED TO DERIVE PREVIOUS PARAME [NUMERIC]
42 008076 1 TYPE OF BAND [CODE TABLE]
204001 ADD ASSOCIATED FIELD
43 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
201129 CHANGE DATA WIDTH
44 999999 1 ASSOCIATED FIELD [NUMERIC]
45 021062 5.84 BACKSCATTER [dB]
201000 CANCEL CHANGE DATA WIDTH
204000 ADD ASSOCIATED FIELD
46 008023 10 FIRST ORDER STATISTICS [CODE TABLE]
47 021062 0.09 BACKSCATTER [dB]
204001 ADD ASSOCIATED FIELD
48 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
201134 CHANGE DATA WIDTH
49 999999 1 ASSOCIATED FIELD [NUMERIC]
50 007001 1353419 HEIGHT OF STATION (SEE NOTE 1) [M]
201000 CANCEL CHANGE DATA WIDTH
204000 ADD ASSOCIATED FIELD
202131 CHANGE SCALE
51 007005 0.75 HEIGHT INCREMENT [M]
202000 CANCEL CHANGE SCALE
52 008023 10 FIRST ORDER STATISTICS [CODE TABLE]
202131 CHANGE SCALE
53 007001 0.904 HEIGHT OF STATION (SEE NOTE 1) [M]
202000 CANCEL CHANGE SCALE
54 021128 19 NUMBER OF VALID POINTS PER SECOND USED TO DERIVE PREVIOUS PARAME [NUMERIC]
204001 ADD ASSOCIATED FIELD
55 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
56 999999 1 ASSOCIATED FIELD [NUMERIC]
57 002173 missing SQUARE OF THE OFF NADIR ANGLE (7) [DEGREE2]
204000 ADD ASSOCIATED FIELD
201130 CHANGE DATA WIDTH
58 002121 18700000000 MEAN FREQUENCY [Hz]
201000 CANCEL CHANGE DATA WIDTH
204001 ADD ASSOCIATED FIELD
59 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
60 999999 1 ASSOCIATED FIELD [NUMERIC]
61 012163 245.83 BRIGHTNESS TEMPERATURE [K]
204000 ADD ASSOCIATED FIELD
201130 CHANGE DATA WIDTH
62 002121 23800000000 MEAN FREQUENCY [Hz]
201000 CANCEL CHANGE DATA WIDTH
204001 ADD ASSOCIATED FIELD
63 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
64 999999 1 ASSOCIATED FIELD [NUMERIC]
65 012163 239.91 BRIGHTNESS TEMPERATURE [K]
204000 ADD ASSOCIATED FIELD
201130 CHANGE DATA WIDTH
66 002121 34000000000 MEAN FREQUENCY [Hz]
201000 CANCEL CHANGE DATA WIDTH
204001 ADD ASSOCIATED FIELD
67 031021 1 ASSOCIATED FIELD SIGNIFICANCE [CODE TABLE]
68 999999 1 ASSOCIATED FIELD [NUMERIC]
69 012163 226.08 BRIGHTNESS TEMPERATURE [K]
204000 ADD ASSOCIATED FIELD
70 002023 8 SATELLITE DERIVED WIND COMPUTATION METHOD [CODE TABLE]
202129 CHANGE SCALE
71 011012 28.39 WIND SPEED AT 10 M [M/S]
202000 CANCEL CHANGE SCALE
72 002023 9 SATELLITE DERIVED WIND COMPUTATION METHOD [CODE TABLE]
202129 CHANGE SCALE
73 011012 40.94 WIND SPEED AT 10 M [M/S]
202000 CANCEL CHANGE SCALE
74 013090 0 RADIOMETER WATER VAPOUR CONTENT [KG/M**2]
75 013091 0 RADIOMETER LIQUID CONTENT [KG/M**2]
Subset 2
...