Message 1 IUSA11 ENMI 100000
Section 0:
Length of BUFR message: 2374
BUFR edition: 4
Section 1:
Length of section: 22
BUFR master table: 0
Originating centre: 88
Originating subcentre: 0
Update sequence number: 0
Optional section present: 0
Data category (table A): 2
International data subcategory: 4
Local data subcategory: 255
Master table version number: 12
Local table version number: 0
Year: 2007
Month: 9
Day: 10
Hour: 0
Minute: 0
Second: 0
Section 3:
Length of section: 9
Number of data subsets: 1
Observed data: 1
Compressed data: 0
Data descriptors unexpanded: 309052
1 001001 1 WMO BLOCK NUMBER [NUMERIC]
2 001002 1 WMO STATION NUMBER [NUMERIC]
3 001011 Jan Mayen SHIP OR MOBILE LAND STATION IDENTIFIER [CCITTIA5]
4 002011 80 RADIOSONDE TYPE [CODE TABLE]
5 002013 4 SOLAR AND INFRARED RADIATION CORRECTION [CODE TABLE]
solar and infrared corrected automatically by radiosonde sy
stem
6 002014 6 TRACKING TECHNIQUE/STATUS OF SYSTEM USED [CODE TABLE]
automatic cross chain loran-c
7 002003 5 TYPE OF MEASURING EQUIPMENT USED [CODE TABLE]
loran c
8 008021 18 TIME SIGNIFICANCE [CODE TABLE]
radiosonde launch time
9 004001 2007 YEAR [YEAR]
10 004002 9 MONTH [MONTH]
11 004003 9 DAY [DAY]
12 004004 23 HOUR [HOUR]
13 004005 11 MINUTE [MINUTE]
14 004006 35 SECOND [SECOND]
15 005001 70.9397 LATITUDE (HIGH ACCURACY) [DEGREE]
16 006001 -8.6679 LONGITUDE (HIGH ACCURACY) [DEGREE]
17 007030 9 HEIGHT OF STATION GROUND ABOVE MEAN SEA LEVEL (SEE NOTE 3) [M]
18 007031 9 HEIGHT OF BAROMETER ABOVE MEAN SEA LEVEL (SEE NOTE 4) [M]
19 007007 9 HEIGHT [M]
20 033024 missing STATION ELEVATION QUALITY MARK (FOR MOBILE STATIONS) [CODE TABLE]
21 008002 7 VERTICAL SIGNIFICANCE (SURFACE OBSERVATIONS) [CODE TABLE]
low cloud
22 020011 3 CLOUD AMOUNT [CODE TABLE]
3 oktas 4/10
23 020013 300 HEIGHT OF BASE OF CLOUD [M]
24 020012 35 CLOUD TYPE [CODE TABLE]
stratocumulus other than stratocumulus cumulogenitus
25 020012 27 CLOUD TYPE [CODE TABLE]
altocumulus translucidus or opacus in two or more layers, or
altocumulus opacus in a single layer, not progressively inv
ading the sky, or altocumulus with altostratus or nimbostrat
us
26 020012 60 CLOUD TYPE [CODE TABLE]
ch clouds invisible owing to darkness, fog, duststorm, sands
torm, or other similar phenomena, or because of a continuous
layer of lower clouds
27 008002 missing VERTICAL SIGNIFICANCE (SURFACE OBSERVATIONS) [CODE TABLE]
28 022043 missing SEA/WATER TEMPERATURE [K]
29 031002 108 EXTENDED DELAYED DESCRIPTOR REPLICATION FACTOR [NUMERIC]
30 004086 0 LONG TIME PERIOD OR DISPLACEMENT [SECOND]
31 008042 145408 EXTENDED VERTICAL SOUNDING SIGNIFICANCE [FLAG TABLE]
=> bit 1 set: surface
=> bit 5 set: significant temperature level
=> bit 6 set: significant humidity level
=> bit 7 set: significant wind level
32 007004 101300 PRESSURE [PA]
33 010009 9 GEOPOTENTIAL HEIGHT [GPM]
34 005015 0.0003 LATITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
35 006015 -0.0021 LONGITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
36 012101 275.8 TEMPERATURE/DRY-BULB TEMPERATURE [K]
37 012103 272.7 DEW-POINT TEMPERATURE [K]
38 011001 354 WIND DIRECTION [DEGREE TRUE]
39 011002 7.2 WIND SPEED [M/S]
40 004086 20 LONG TIME PERIOD OR DISPLACEMENT [SECOND]
41 008042 2048 EXTENDED VERTICAL SOUNDING SIGNIFICANCE [FLAG TABLE]
=> bit 7 set: significant wind level
42 007004 100010 PRESSURE [PA]
43 010009 112 GEOPOTENTIAL HEIGHT [GPM]
44 005015 0.0003 LATITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
45 006015 -0.0021 LONGITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
46 012101 275.1 TEMPERATURE/DRY-BULB TEMPERATURE [K]
47 012103 272.7 DEW-POINT TEMPERATURE [K]
48 011001 76 WIND DIRECTION [DEGREE TRUE]
49 011002 12.1 WIND SPEED [M/S]
50 004086 20 LONG TIME PERIOD OR DISPLACEMENT [SECOND]
51 008042 65536 EXTENDED VERTICAL SOUNDING SIGNIFICANCE [FLAG TABLE]
=> bit 2 set: standard level
52 007004 100000 PRESSURE [PA]
53 010009 114 GEOPOTENTIAL HEIGHT [GPM]
54 005015 0.0003 LATITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
55 006015 -0.0021 LONGITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
56 012101 275.1 TEMPERATURE/DRY-BULB TEMPERATURE [K]
57 012103 272.7 DEW-POINT TEMPERATURE [K]
58 011001 76 WIND DIRECTION [DEGREE TRUE]
59 011002 12.1 WIND SPEED [M/S]
60 004086 28 LONG TIME PERIOD OR DISPLACEMENT [SECOND]
61 008042 2048 EXTENDED VERTICAL SOUNDING SIGNIFICANCE [FLAG TABLE]
=> bit 7 set: significant wind level
62 007004 99480 PRESSURE [PA]
...
1100 004086 8216 LONG TIME PERIOD OR DISPLACEMENT [SECOND]
1101 008042 14336 EXTENDED VERTICAL SOUNDING SIGNIFICANCE [FLAG TABLE]
=> bit 5 set: significant temperature level
=> bit 6 set: significant humidity level
=> bit 7 set: significant wind level
1102 007004 410 PRESSURE [PA]
1103 010009 37183 GEOPOTENTIAL HEIGHT [GPM]
1104 005015 -0.5197 LATITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
1105 006015 2.2479 LONGITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
1106 012101 238.4 TEMPERATURE/DRY-BULB TEMPERATURE [K]
1107 012103 199.9 DEW-POINT TEMPERATURE [K]
1108 011001 3 WIND DIRECTION [DEGREE TRUE]
1109 011002 8.4 WIND SPEED [M/S]
1110 031001 1 DELAYED DESCRIPTOR REPLICATION FACTOR [NUMERIC]
1111 004086 2158 LONG TIME PERIOD OR DISPLACEMENT [SECOND]
1112 008042 18432 EXTENDED VERTICAL SOUNDING SIGNIFICANCE [FLAG TABLE]
=> bit 4 set: maximum wind level
=> bit 7 set: significant wind level
1113 007004 25510 PRESSURE [PA]
1114 005015 -0.1797 LATITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
1115 006015 0.3379 LONGITUDE DISPLACEMENT (HIGH ACCURACY) [DEGREE]
1116 011061 9.3 ABSOLUTE WIND SHEAR IN 1 KM LAYER BELOW [M/S]
1117 011062 3 ABSOLUTE WIND SHEAR IN 1 KM LAYER ABOVE [M/S]