002002 TYPE OF INSTRUMENTATION FOR WIND MEASUREMENT FLAG TABLE 2002
0 -> MEASURED IN M S-1 UNLESS OTHERWISE INDICATED
1 -> CERTIFIED INSTRUMENTS
2 -> ORIGINALY MEASURED IN KNOTS
3 -> ORIGINALY MEASURED IN KM/H
002016 RADIOSONDE CONFIGURATION FLAG TABLE 2016
1 -> TRAIN REGULATOR
2 -> LIGHT UNIT
3 -> PARACHUTE
4 -> ROOFTOP RELEASE
002021 SATELLITE INSTRUMENT DATA USED IN PROCESSING FLAG TABLE 2021
1 -> HIGH RESOLUTION INFRA RED SOUNDER (HIRS)
2 -> MICROWAVE SOUNDING UNIT (MSU )
3 -> STRATOSPHERIC SOUNDING UNIT (SSU)
4 -> AMI WIND MODE
5 -> AMI WAVE MODE
6 -> AMI IMAGE MODE
7 -> RADAR ALTIMETER
8 -> ATSR
002022 SATELLITE DATA-PROCESSING TECHNIQUE USED FLAG TABLE 2022
1 -> PROCESSING TECHNIQUE NOT DEFINED
2 -> AUTOMATED STATISTICAL REGRESSION
3 -> CLEAR PATH
4 -> PARTLY CLOUDY PATH
5 -> CLOUDY PATH
002025 SATELLITE CHANNEL(S) USED IN COMPUTATION FLAG TABLE 2025
2 -> HIRS
...